# Change log - AutoConnect for ESP8266/ESP32
ESP8266/ESP32 WLAN configuration at run time with web interface
Author: Hieromon Ikasamo

Skip to content

# Change log

#### [0.9.7] Jan. 25, 2019

- Fixed crash in some environments. Thank you @ageurtse
- Supports AutoConnect menu extention by user sketch with AutoConnectAux.
- Supports loading and saving of user-defined parameters with JSON format.
- Improved the WiFi connection sequence at the first WiFi.begin. Even if AutoConnectConfig::autoReconnect is disabled when SSID and PSK are not specified, it will use the information of the last established access point. The autoReconnect option will achieve trying the connect after a previous connection failed.
- Supports the AutoConnectConfig::immediateStart option and immediately starts the portal without first trying WiFi.begin. You can start the captive portal at any time in combination with the AutoConnectConfig::autoRise option.
- Improved boot uri after reset. AutoConnectConfig::bootUri can be specified either /_ac or HOME path as the uri to be accessed after invoking Reset from AutoConnect menu.
- Improved source code placement of predefined macros. Defined common macros have been moved to `AutoConnectDefs.h`.
- Supports AutoConnectConfig::hostName. It activates `WiFi.hostname()`/`WiFi.setHostName()`.
- Supports the captive portal time-out. It can be controlled by AutoConnectConfig::portalTimeout and AutoConnectConfig::retainPortal.

#### [0.9.6] Sept.27, 2018.

- Improvement of RSSI detection for saved SSIDs.
- Fixed disconnection SoftAP completely at the first connection phase of the AutoConnect::begin.

#### [0.9.5] Aug.27, 2018.

- Supports ESP32.
- Fixed that crash may occur if the number of stored credentials in the EEPROM is smaller than the number of found WiFi networks.

#### [0.9.4] May 5, 2018.

- Automatically focus passphrase after selecting SSID with Configure New AP.
- Supports AutoConnectConfig::autoReconnect option, it will scan the WLAN when it can not connect to the default SSID, apply the applicable credentials if it is saved, and try reconnecting.

#### [0.9.3] March 23, 2018.

- Supports a static IP address assignment.

#### [0.9.2] March 19, 2018.

- Improvement of string literal declaration with the examples, no library change.

#### [0.9.1] March 13, 2018.

- A release of the stable.