@prefix atom:  <http://lv2plug.in/ns/ext/atom#> .
@prefix doap: <http://usefulinc.com/ns/doap#>.
@prefix foaf: <http://xmlns.com/foaf/0.1/> .
@prefix ll:   <http://ll-plugins.nongnu.org/lv2/namespace#>.
@prefix lv2:  <http://lv2plug.in/ns/lv2core#>.
@prefix pg:   <http://ll-plugins.nongnu.org/lv2/ext/portgroups#>.
@prefix rdf:  <http://www.w3.org/1999/02/22-rdf-syntax-ns#>.
@prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#>.
@prefix ui:    <http://lv2plug.in/ns/extensions/ui#>.
@prefix urid:  <http://lv2plug.in/ns/ext/urid#>.
@prefix epp: <http://lv2plug.in/ns/dev/extportinfo#>.
@prefix pprops: <http://lv2plug.in/ns/ext/port-props#>.
@prefix pset: <http://lv2plug.in/ns/ext/presets#> .

<https://github.com/dcoredump/dexed.lv2>
    a lv2:InstrumentPlugin, lv2:Plugin ;
    lv2:binary <dexed.so> ;
    ll:pegName "p";

    lv2:port [
        a lv2:InputPort, atom:AtomPort ;
        atom:bufferType atom:Sequence ;
        atom:supports <http://lv2plug.in/ns/ext/midi#MidiEvent>,
                      <http://lv2plug.in/ns/ext/patch#Message> ;
        lv2:index 0 ;
        lv2:symbol "midi_in" ;
        lv2:name "MIDI Input" ;
    ] ,
    [
        a lv2:OutputPort, lv2:AudioPort ;
        lv2:index 1 ;
        lv2:symbol "audio_out" ;
        lv2:name "Audio Output" ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 2 ;
        lv2:symbol "cutoff" ;
        lv2:name "Cutoff" ;
        lv2:default 1.000000 ;
        lv2:minimum 0.0 ;
        lv2:maximum 1.0 ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 3 ;
        lv2:symbol "resonance" ;
        lv2:name "Resonance" ;
        lv2:default 0.000000 ;
        lv2:minimum 0.0 ;
        lv2:maximum 1.0 ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 4 ;
        lv2:symbol "output" ;
        lv2:name "Gain" ;
        lv2:default 1.000000 ;
        lv2:minimum 0.0 ;
        lv2:maximum 2.0 ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 5 ;
        lv2:symbol "engine" ;
        lv2:name "ENGINE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 2 ;
	lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "MSFA" ;
            rdfs:comment "MSFA" ;
        ], [
            rdf:value 1 ;
            rdfs:label "Mark I" ;
            rdfs:comment "Mark I" ;
        ], [
            rdf:value 2 ;
            rdfs:label "OPL" ;
            rdfs:comment "OPL" ;
	];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 6 ;
        lv2:symbol "polymono" ;
        lv2:name "POLY-MONO" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
	lv2:portProperty lv2:toggled, lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 7 ;
        lv2:symbol "pitch_bend_range" ;
        lv2:name "PB RANGE" ;
        lv2:default 1 ;
        lv2:minimum 0 ;
        lv2:maximum 12 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 8 ;
        lv2:symbol "pitch_bend_step" ;
        lv2:name "PB STEP" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 12 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 9 ;
        lv2:symbol "mod_wheel_range" ;
        lv2:name "MW RANGE" ;
        lv2:default 99 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 10 ;
        lv2:symbol "mod_wheel_assign" ;
        lv2:name "MW ASSIGN" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Off" ;
            rdfs:comment "Off" ;
        ], [
            rdf:value 1 ;
            rdfs:label "Pitch" ;
            rdfs:comment "Pitch" ;
        ], [
            rdf:value 2 ;
            rdfs:label "Amp" ;
            rdfs:comment "Amp" ;
        ], [
            rdf:value 3 ;
            rdfs:label "Amp+Pitch" ;
            rdfs:comment "Amp+Pitch" ;
        ], [
            rdf:value 4 ;
            rdfs:label "EG" ;
            rdfs:comment "EG" ;
        ], [
            rdf:value 5 ;
            rdfs:label "EG+Pitch" ;
            rdfs:comment "EG+Pitch" ;
        ], [
            rdf:value 6 ;
            rdfs:label "EG+Amp" ;
            rdfs:comment "EG+Amp" ;
        ], [
            rdf:value 7 ;
            rdfs:label "EG+Pitch+Amp" ;
            rdfs:comment "EG+Pitch+Amp" ;
	];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 11 ;
        lv2:symbol "foot_ctrl_range" ;
        lv2:name "FC RANGE" ;
        lv2:default 99 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 12 ;
        lv2:symbol "foot_ctrl_assign" ;
        lv2:name "FC ASSIGN" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Off" ;
            rdfs:comment "Off" ;
        ], [
            rdf:value 1 ;
            rdfs:label "Pitch" ;
            rdfs:comment "Pitch" ;
        ], [
            rdf:value 2 ;
            rdfs:label "Amp" ;
            rdfs:comment "Amp" ;
        ], [
            rdf:value 3 ;
            rdfs:label "Amp+Pitch" ;
            rdfs:comment "Amp+Pitch" ;
        ], [
            rdf:value 4 ;
            rdfs:label "EG" ;
            rdfs:comment "EG" ;
        ], [
            rdf:value 5 ;
            rdfs:label "EG+Pitch" ;
            rdfs:comment "EG+Pitch" ;
        ], [
            rdf:value 6 ;
            rdfs:label "EG+Amp" ;
            rdfs:comment "EG+Amp" ;
        ], [
            rdf:value 7 ;
            rdfs:label "EG+Pitch+Amp" ;
            rdfs:comment "EG+Pitch+Amp" ;
	];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 13 ;
        lv2:symbol "breath_ctrl_range" ;
        lv2:name "BC RANGE" ;
        lv2:default 99 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 14 ;
        lv2:symbol "breath_ctrl_assign" ;
        lv2:name "BC ASSIGN" ;
        lv2:default 0;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Off" ;
            rdfs:comment "Off" ;
        ], [
            rdf:value 1 ;
            rdfs:label "Pitch" ;
            rdfs:comment "Pitch" ;
        ], [
            rdf:value 2 ;
            rdfs:label "Amp" ;
            rdfs:comment "Amp" ;
        ], [
            rdf:value 3 ;
            rdfs:label "Amp+Pitch" ;
            rdfs:comment "Amp+Pitch" ;
        ], [
            rdf:value 4 ;
            rdfs:label "EG" ;
            rdfs:comment "EG" ;
        ], [
            rdf:value 5 ;
            rdfs:label "EG+Pitch" ;
            rdfs:comment "EG+Pitch" ;
        ], [
            rdf:value 6 ;
            rdfs:label "EG+Amp" ;
            rdfs:comment "EG+Amp" ;
        ], [
            rdf:value 7 ;
            rdfs:label "EG+Pitch+Amp" ;
            rdfs:comment "EG+Pitch+Amp" ;
	];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 15 ;
        lv2:symbol "aftertouch_range" ;
        lv2:name "AT RANGE" ;
        lv2:default 99 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 16 ;
        lv2:symbol "aftertouch_assign" ;
        lv2:name "AT ASSIGN" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Off" ;
            rdfs:comment "Off" ;
        ], [
            rdf:value 1 ;
            rdfs:label "Pitch" ;
            rdfs:comment "Pitch" ;
        ], [
            rdf:value 2 ;
            rdfs:label "Amp" ;
            rdfs:comment "Amp" ;
        ], [
            rdf:value 3 ;
            rdfs:label "Amp+Pitch" ;
            rdfs:comment "Amp+Pitch" ;
        ], [
            rdf:value 4 ;
            rdfs:label "EG" ;
            rdfs:comment "EG" ;
        ], [
            rdf:value 5 ;
            rdfs:label "EG+Pitch" ;
            rdfs:comment "EG+Pitch" ;
        ], [
            rdf:value 6 ;
            rdfs:label "EG+Amp" ;
            rdfs:comment "EG+Amp" ;
        ], [
            rdf:value 7 ;
            rdfs:label "EG+Pitch+Amp" ;
            rdfs:comment "EG+Pitch+Amp" ;
	];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 17 ;
        lv2:symbol "master_tune" ;
        lv2:name "MASTER TUNE" ;
        lv2:default 0.0 ;
        lv2:minimum -1.0 ;
        lv2:maximum 1.0 ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 18 ;
        lv2:symbol "algorithm_num" ;
        lv2:name "ALGORITHM" ;
        lv2:default 5 ;
        lv2:minimum 1 ;
        lv2:maximum 32 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 19 ;
        lv2:symbol "feedback" ;
        lv2:name "FEEDBACK" ;
        lv2:default 6 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 20 ;
        lv2:symbol "oscillator_sync" ;
        lv2:name "OSC KEY SYNC" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
	lv2:portProperty lv2:toggled, lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 21 ;
        lv2:symbol "lfo_speed" ;
        lv2:name "LFO SPEED" ;
        lv2:default 34 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 22 ;
        lv2:symbol "lfo_delay" ;
        lv2:name "LFO DELAY" ;
        lv2:default 33 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 23 ;
        lv2:symbol "lfo_pitch_mod_depth" ;
        lv2:name "LFO PM DEPTH" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 24 ;
        lv2:symbol "lfo_amp_mod_depth" ;
        lv2:name "LFO AM DEPTH" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 25 ;
        lv2:symbol "lfo_sync" ;
        lv2:name "LFO KEY SYNC" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
	lv2:portProperty lv2:toggled, lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 26 ;
        lv2:symbol "lfo_waveform" ;
        lv2:name "LFO WAVE" ;
        lv2:default 4 ;
        lv2:minimum 0 ;
        lv2:maximum 5 ;
	lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Triangle" ;
            rdfs:comment "Triangle" ;
        ], [
            rdf:value 1 ;
            rdfs:label "Saw-Down" ;
            rdfs:comment "Saw-Down" ;
        ], [
            rdf:value 2 ;
            rdfs:label "Saw-Up" ;
            rdfs:comment "Saw-Up" ;
        ], [
            rdf:value 3 ;
            rdfs:label "Square" ;
            rdfs:comment "Square" ;
        ], [
            rdf:value 4 ;
            rdfs:label "Sine" ;
            rdfs:comment "Sine" ;
        ], [
            rdf:value 6 ;
            rdfs:label "Sample & Hold" ;
            rdfs:comment "Sample & Hold" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 27 ;
        lv2:symbol "transpose" ;
        lv2:name "MIDDLE C" ;
        lv2:default 24 ;
        lv2:minimum 0 ;
        lv2:maximum 48 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 28 ;
        lv2:symbol "pitch_mod_sensitivity" ;
        lv2:name "P MODE SENS." ;
        lv2:default 3 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 29 ;
        lv2:symbol "pitch_eg_rate_1" ;
        lv2:name "PITCH EG RATE 1" ;
        lv2:default 94 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 30 ;
        lv2:symbol "pitch_eg_rate_2" ;
        lv2:name "PITCH EG RATE 2" ;
        lv2:default 67 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 31 ;
        lv2:symbol "pitch_eg_rate_3" ;
        lv2:name "PITCH EG RATE 3" ;
        lv2:default 95 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 32 ;
        lv2:symbol "pitch_eg_rate_4" ;
        lv2:name "PITCH EG RATE 4" ;
        lv2:default 60 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 33 ;
        lv2:symbol "pitch_eg_level_1" ;
        lv2:name "PITCH EG LEVEL 1" ;
        lv2:default 50 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 34 ;
        lv2:symbol "pitch_eg_level_2" ;
        lv2:name "PITCH EG LEVEL 2" ;
        lv2:default 50 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 35 ;
        lv2:symbol "pitch_eg_level_3" ;
        lv2:name "PITCH EG LEVEL 3" ;
        lv2:default 50 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 36 ;
        lv2:symbol "pitch_eg_level_4" ;
        lv2:name "PITCH EG LEVEL 4" ;
        lv2:default 50 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 37 ;
        lv2:symbol "op1_eg_rate_1" ;
        lv2:name "OP1 EG RATE 1" ;
        lv2:default 96 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 38 ;
        lv2:symbol "op1_eg_rate_2" ;
        lv2:name "OP1 EG RATE 2" ;
        lv2:default 25 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 39 ;
        lv2:symbol "op1_eg_rate_3" ;
        lv2:name "OP1 EG RATE 3" ;
        lv2:default 25 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 40 ;
        lv2:symbol "op1_eg_rate_4" ;
        lv2:name "OP1 EG RATE 4" ;
        lv2:default 67 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 41 ;
        lv2:symbol "op1_eg_level_1" ;
        lv2:name "OP1 EG LEVEL 1" ;
        lv2:default 99 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 42 ;
        lv2:symbol "op1_eg_level_2" ;
        lv2:name "OP1 EG LEVEL 2" ;
        lv2:default 75 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 43 ;
        lv2:symbol "op1_eg_level_3" ;
        lv2:name "OP1 EG LEVEL 3" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 44 ;
        lv2:symbol "op1_eg_level_4" ;
        lv2:name "OP1 EG LEVEL 4" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 45 ;
        lv2:symbol "op1_operator_output_level" ;
        lv2:name "OP1 OUTPUT LEVEL" ;
        lv2:default 99 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 46 ;
        lv2:symbol "op1_osc_mode" ;
        lv2:name "OP1 MODE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
	lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Ratio" ;
            rdfs:comment "Ratio" ;
        ], [
            rdf:value 1 ;
            rdfs:label "Fixed" ;
            rdfs:comment "Fixed" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 47 ;
        lv2:symbol "op1_osc_freq_coarse" ;
        lv2:name "OP1 F COARSE" ;
        lv2:default 1 ;
        lv2:minimum 0 ;
        lv2:maximum 31 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 48 ;
        lv2:symbol "op1_osc_freq_fine" ;
        lv2:name "OP1 F FINE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 49 ;
        lv2:symbol "op1_osc_detune" ;
        lv2:name "OP1 OSC DETUNE" ;
        lv2:default 3 ;
        lv2:minimum -7 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 50 ;
        lv2:symbol "op1_kbd_lev_scl_brk_pt" ;
        lv2:name "OP1 BREAK POINT" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 51 ;
        lv2:symbol "op1_kbd_lev_scl_lft_depth" ;
        lv2:name "OP1 L SCALE DEPTH" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 52 ;
        lv2:symbol "op1_kbd_lev_scl_rht_depth" ;
        lv2:name "OP1 R SCALE DEPTH" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 53 ;
        lv2:symbol "op1_kbd_lev_scl_lft_curve" ;
        lv2:name "OP1 L KEY CURVE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
	lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "-LIN" ;
            rdfs:comment "-LIN" ;
        ], [
            rdf:value 1 ;
            rdfs:label "-EXP" ;
            rdfs:comment "-EXP" ;
        ], [
            rdf:value 2 ;
            rdfs:label "+EXP" ;
            rdfs:comment "+EXP" ;
        ], [
            rdf:value 3 ;
            rdfs:label "+LIN" ;
            rdfs:comment "+LIN" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 54 ;
        lv2:symbol "op1_kbd_lev_scl_rht_curve" ;
        lv2:name "OP1 R KEY CURVE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
	lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "-LIN" ;
            rdfs:comment "-LIN" ;
        ], [
            rdf:value 1 ;
            rdfs:label "-EXP" ;
            rdfs:comment "-EXP" ;
        ], [
            rdf:value 2 ;
            rdfs:label "+EXP" ;
            rdfs:comment "+EXP" ;
        ], [
            rdf:value 3 ;
            rdfs:label "+LIN" ;
            rdfs:comment "+LIN" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 55 ;
        lv2:symbol "op1_kbd_rate_scaling" ;
        lv2:name "OP1 RATE SCALING" ;
        lv2:default 3 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 56 ;
        lv2:symbol "op1_amp_mod_sensitivity" ;
        lv2:name "OP1 A MOD SENS." ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 57 ;
        lv2:symbol "op1_key_vel_sensitivity" ;
        lv2:name "OP1 KEY VELOCITY" ;
        lv2:default 2 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 58 ;
        lv2:symbol "op2_eg_rate_1" ;
        lv2:name "OP2 EG RATE 1" ;
        lv2:default 95 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 59 ;
        lv2:symbol "op2_eg_rate_2" ;
        lv2:name "OP2 EG RATE 2" ;
        lv2:default 50 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 60 ;
        lv2:symbol "op2_eg_rate_3" ;
        lv2:name "OP2 EG RATE 3" ;
        lv2:default 35 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 61 ;
        lv2:symbol "op2_eg_rate_4" ;
        lv2:name "OP2 EG RATE 4" ;
        lv2:default 78 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 62 ;
        lv2:symbol "op2_eg_level_1" ;
        lv2:name "OP2 EG LEVEL 1" ;
        lv2:default 99 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 63 ;
        lv2:symbol "op2_eg_level_2" ;
        lv2:name "OP2 EG LEVEL 2" ;
        lv2:default 75 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 64 ;
        lv2:symbol "op2_eg_level_3" ;
        lv2:name "OP2 EG LEVEL 3" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 65 ;
        lv2:symbol "op2_eg_level_4" ;
        lv2:name "OP2 EG LEVEL 4" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 66 ;
        lv2:symbol "op2_operator_output_level" ;
        lv2:name "OP2 OUTPUT LEVEL" ;
        lv2:default 58 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 67 ;
        lv2:symbol "op2_osc_mode" ;
        lv2:name "OP2 MODE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Ratio" ;
            rdfs:comment "Ratio" ;
        ], [
            rdf:value 1 ;
            rdfs:label "Fixed" ;
            rdfs:comment "Fixed" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 68 ;
        lv2:symbol "op2_osc_freq_coarse" ;
        lv2:name "OP2 F COARSE" ;
        lv2:default 14 ;
        lv2:minimum 0 ;
        lv2:maximum 31 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 69 ;
        lv2:symbol "op2_osc_freq_fine" ;
        lv2:name "OP2 F FINE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 100 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 70 ;
        lv2:symbol "op2_osc_detune" ;
        lv2:name "OP2 OSC DETUNE" ;
        lv2:default 0 ;
        lv2:minimum -7 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 71 ;
        lv2:symbol "op2_kbd_lev_scl_brk_pt" ;
        lv2:name "OP2 BREAK POINT" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 100 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 72 ;
        lv2:symbol "op2_kbd_lev_scl_lft_depth" ;
        lv2:name "OP2 L SCALE DEPTH" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 100 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 73 ;
        lv2:symbol "op2_kbd_lev_scl_rht_depth" ;
        lv2:name "OP2 R SCALE DEPTH" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 100 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 74 ;
        lv2:symbol "op2_kbd_lev_scl_lft_curve" ;
        lv2:name "OP2 L KEY CURVE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
	lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "-LIN" ;
            rdfs:comment "-LIN" ;
        ], [
            rdf:value 1 ;
            rdfs:label "-EXP" ;
            rdfs:comment "-EXP" ;
        ], [
            rdf:value 2 ;
            rdfs:label "+EXP" ;
            rdfs:comment "+EXP" ;
        ], [
            rdf:value 3 ;
            rdfs:label "+LIN" ;
            rdfs:comment "+LIN" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 75 ;
        lv2:symbol "op2_kbd_lev_scl_rht_curve" ;
        lv2:name "OP2 R KEY CURVE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "-LIN" ;
            rdfs:comment "-LIN" ;
        ], [
            rdf:value 1 ;
            rdfs:label "-EXP" ;
            rdfs:comment "-EXP" ;
        ], [
            rdf:value 2 ;
            rdfs:label "+EXP" ;
            rdfs:comment "+EXP" ;
        ], [
            rdf:value 3 ;
            rdfs:label "+LIN" ;
            rdfs:comment "+LIN" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 76 ;
        lv2:symbol "op2_kbd_rate_scaling" ;
        lv2:name "OP2 RATE SCALING" ;
        lv2:default 3 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 77 ;
        lv2:symbol "op2_amp_mod_sensitivity" ;
        lv2:name "OP2 A MOD SENS." ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 78 ;
        lv2:symbol "op2_key_vel_sensitivity" ;
        lv2:name "OP2 KEY VELOCITY" ;
        lv2:default 7 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 79 ;
        lv2:symbol "op3_eg_rate_1" ;
        lv2:name "OP3 EG RATE 1" ;
        lv2:default 95 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 80 ;
        lv2:symbol "op3_eg_rate_2" ;
        lv2:name "OP3 EG RATE 2" ;
        lv2:default 20 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 81 ;
        lv2:symbol "op3_eg_rate_3" ;
        lv2:name "OP3 EG RATE 3" ;
        lv2:default 20 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 82 ;
        lv2:symbol "op3_eg_rate_4" ;
        lv2:name "OP3 EG RATE 4" ;
        lv2:default 50 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 83 ;
        lv2:symbol "op3_eg_level_1" ;
        lv2:name "OP3 EG LEVEL 1" ;
        lv2:default 99 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 84 ;
        lv2:symbol "op3_eg_level_2" ;
        lv2:name "OP3 EG LEVEL 2" ;
        lv2:default 95 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 85 ;
        lv2:symbol "op3_eg_level_3" ;
        lv2:name "OP3 EG LEVEL 3" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 86 ;
        lv2:symbol "op3_eg_level_4" ;
        lv2:name "OP3 EG LEVEL 4" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 87 ;
        lv2:symbol "op3_operator_output_level" ;
        lv2:name "OP3 OUTPUT LEVEL" ;
        lv2:default 99 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 88 ;
        lv2:symbol "op3_osc_mode" ;
        lv2:name "OP3 MODE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Ratio" ;
            rdfs:comment "Ratio" ;
        ], [
            rdf:value 1 ;
            rdfs:label "Fixed" ;
            rdfs:comment "Fixed" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 89 ;
        lv2:symbol "op3_osc_freq_coarse" ;
        lv2:name "OP3 F COARSE" ;
        lv2:default 1 ;
        lv2:minimum 0 ;
        lv2:maximum 31 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 90 ;
        lv2:symbol "op3_osc_freq_fine" ;
        lv2:name "OP3 F FINE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 91 ;
        lv2:symbol "op3_osc_detune" ;
        lv2:name "OP3 OSC DETUNE" ;
        lv2:default 0 ;
        lv2:minimum -7 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 92 ;
        lv2:symbol "op3_kbd_lev_scl_brk_pt" ;
        lv2:name "OP3 BREAK POINT" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 93 ;
        lv2:symbol "op3_kbd_lev_scl_lft_depth" ;
        lv2:name "OP3 L SCALE DEPTH" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 94 ;
        lv2:symbol "op3_kbd_lev_scl_rht_depth" ;
        lv2:name "OP3 R SCALE DEPTH" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 95 ;
        lv2:symbol "op3_kbd_lev_scl_lft_curve" ;
        lv2:name "OP3 L KEY CURVE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "-LIN" ;
            rdfs:comment "-LIN" ;
        ], [
            rdf:value 1 ;
            rdfs:label "-EXP" ;
            rdfs:comment "-EXP" ;
        ], [
            rdf:value 2 ;
            rdfs:label "+EXP" ;
            rdfs:comment "+EXP" ;
        ], [
            rdf:value 3 ;
            rdfs:label "+LIN" ;
            rdfs:comment "+LIN" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 96 ;
        lv2:symbol "op3_kbd_lev_scl_rht_curve" ;
        lv2:name "OP3 R KEY CURVE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "-LIN" ;
            rdfs:comment "-LIN" ;
        ], [
            rdf:value 1 ;
            rdfs:label "-EXP" ;
            rdfs:comment "-EXP" ;
        ], [
            rdf:value 2 ;
            rdfs:label "+EXP" ;
            rdfs:comment "+EXP" ;
        ], [
            rdf:value 3 ;
            rdfs:label "+LIN" ;
            rdfs:comment "+LIN" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 97 ;
        lv2:symbol "op3_kbd_rate_scaling" ;
        lv2:name "OP3 RATE SCALING" ;
        lv2:default 3 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 98 ;
        lv2:symbol "op3_amp_mod_sensitivity" ;
        lv2:name "OP3 A MOD SENS." ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 99 ;
        lv2:symbol "op3_key_vel_sensitivity" ;
        lv2:name "OP3 KEY VELOCITY" ;
        lv2:default 2 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 100 ;
        lv2:symbol "op4_eg_rate_1" ;
        lv2:name "OP4 EG RATE 1" ;
        lv2:default 95 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 101 ;
        lv2:symbol "op4_eg_rate_2" ;
        lv2:name "OP4 EG RATE 2" ;
        lv2:default 29 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 102 ;
        lv2:symbol "op4_eg_rate_3" ;
        lv2:name "OP4 EG RATE 3" ;
        lv2:default 20 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 103 ;
        lv2:symbol "op4_eg_rate_4" ;
        lv2:name "OP4 EG RATE 4" ;
        lv2:default 50 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 104 ;
        lv2:symbol "op4_eg_level_1" ;
        lv2:name "OP4 EG LEVEL 1" ;
        lv2:default 99 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 105 ;
        lv2:symbol "op4_eg_level_2" ;
        lv2:name "OP4 EG LEVEL 2" ;
        lv2:default 95 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 106 ;
        lv2:symbol "op4_eg_level_3" ;
        lv2:name "OP4 EG LEVEL 3" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 107 ;
        lv2:symbol "op4_eg_level_4" ;
        lv2:name "OP4 EG LEVEL 4" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 108 ;
        lv2:symbol "op4_operator_output_level" ;
        lv2:name "OP4 OUTPUT LEVEL" ;
        lv2:default 89 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 109 ;
        lv2:symbol "op4_osc_mode" ;
        lv2:name "OP4 MODE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Ratio" ;
            rdfs:comment "Ratio" ;
        ], [
            rdf:value 1 ;
            rdfs:label "Fixed" ;
            rdfs:comment "Fixed" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 110 ;
        lv2:symbol "op4_osc_freq_coarse" ;
        lv2:name "OP4 F COARSE" ;
        lv2:default 1 ;
        lv2:minimum 0 ;
        lv2:maximum 31 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 111 ;
        lv2:symbol "op4_osc_freq_fine" ;
        lv2:name "OP4 F FINE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 112 ;
        lv2:symbol "op4_osc_detune" ;
        lv2:name "OP4 OSC DETUNE" ;
        lv2:default 0 ;
        lv2:minimum -7 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 113 ;
        lv2:symbol "op4_kbd_lev_scl_brk_pt" ;
        lv2:name "OP4 BREAK POINT" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 114 ;
        lv2:symbol "op4_kbd_lev_scl_lft_depth" ;
        lv2:name "OP4 L SCALE DEPTH" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 115 ;
        lv2:symbol "op4_kbd_lev_scl_rht_depth" ;
        lv2:name "OP4 R SCALE DEPTH" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 116 ;
        lv2:symbol "op4_kbd_lev_scl_lft_curve" ;
        lv2:name "OP4 L KEY CURVE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "-LIN" ;
            rdfs:comment "-LIN" ;
        ], [
            rdf:value 1 ;
            rdfs:label "-EXP" ;
            rdfs:comment "-EXP" ;
        ], [
            rdf:value 2 ;
            rdfs:label "+EXP" ;
            rdfs:comment "+EXP" ;
        ], [
            rdf:value 3 ;
            rdfs:label "+LIN" ;
            rdfs:comment "+LIN" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 117 ;
        lv2:symbol "op4_kbd_lev_scl_rht_curve" ;
        lv2:name "OP4 R KEY CURVE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "-LIN" ;
            rdfs:comment "-LIN" ;
        ], [
            rdf:value 1 ;
            rdfs:label "-EXP" ;
            rdfs:comment "-EXP" ;
        ], [
            rdf:value 2 ;
            rdfs:label "+EXP" ;
            rdfs:comment "+EXP" ;
        ], [
            rdf:value 3 ;
            rdfs:label "+LIN" ;
            rdfs:comment "+LIN" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 118 ;
        lv2:symbol "op4_kbd_rate_scaling" ;
        lv2:name "OP4 RATE SCALING" ;
        lv2:default 3 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 119 ;
        lv2:symbol "op4_amp_mod_sensitivity" ;
        lv2:name "OP4 A MOD SENS." ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 120 ;
        lv2:symbol "op4_key_vel_sensitivity" ;
        lv2:name "OP4 KEY VELOCITY" ;
        lv2:default 6 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 121 ;
        lv2:symbol "op5_eg_rate_1" ;
        lv2:name "OP5 EG RATE 1" ;
        lv2:default 95 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 122 ;
        lv2:symbol "op5_eg_rate_2" ;
        lv2:name "OP5 EG RATE 2" ;
        lv2:default 20 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 123 ;
        lv2:symbol "op5_eg_rate_3" ;
        lv2:name "OP5 EG RATE 3" ;
        lv2:default 20 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 124 ;
        lv2:symbol "op5_eg_rate_4" ;
        lv2:name "OP5 EG RATE 4" ;
        lv2:default 50 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 125 ;
        lv2:symbol "op5_eg_level_1" ;
        lv2:name "OP5 EG LEVEL 1" ;
        lv2:default 99 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 126 ;
        lv2:symbol "op5_eg_level_2" ;
        lv2:name "OP5 EG LEVEL 2" ;
        lv2:default 95 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 127 ;
        lv2:symbol "op5_eg_level_3" ;
        lv2:name "OP5 EG LEVEL 3" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 128 ;
        lv2:symbol "op5_eg_level_4" ;
        lv2:name "OP5 EG LEVEL 4" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 129 ;
        lv2:symbol "op5_operator_output_level" ;
        lv2:name "OP5 OUTPUT LEVEL" ;
        lv2:default 99 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 130 ;
        lv2:symbol "op5_osc_mode" ;
        lv2:name "OP5 MODE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Ratio" ;
            rdfs:comment "Ratio" ;
        ], [
            rdf:value 1 ;
            rdfs:label "Fixed" ;
            rdfs:comment "Fixed" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 131 ;
        lv2:symbol "op5_osc_freq_coarse" ;
        lv2:name "OP5 F COARSE" ;
        lv2:default 1 ;
        lv2:minimum 0 ;
        lv2:maximum 31 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 132 ;
        lv2:symbol "op5_osc_freq_fine" ;
        lv2:name "OP5 F FINE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 133 ;
        lv2:symbol "op5_osc_detune" ;
        lv2:name "OP5 OSC DETUNE" ;
        lv2:default -7 ;
        lv2:minimum -7 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 134 ;
        lv2:symbol "op5_kbd_lev_scl_brk_pt" ;
        lv2:name "OP5 BREAK POINT" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 135 ;
        lv2:symbol "op5_kbd_lev_scl_lft_depth" ;
        lv2:name "OP5 L SCALE DEPTH" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 136 ;
        lv2:symbol "op5_kbd_lev_scl_rht_depth" ;
        lv2:name "OP5 R SCALE DEPTH" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 137 ;
        lv2:symbol "op5_kbd_lev_scl_lft_curve" ;
        lv2:name "OP5 L KEY CURVE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "-LIN" ;
            rdfs:comment "-LIN" ;
        ], [
            rdf:value 1 ;
            rdfs:label "-EXP" ;
            rdfs:comment "-EXP" ;
        ], [
            rdf:value 2 ;
            rdfs:label "+EXP" ;
            rdfs:comment "+EXP" ;
        ], [
            rdf:value 3 ;
            rdfs:label "+LIN" ;
            rdfs:comment "+LIN" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 138 ;
        lv2:symbol "op5_kbd_lev_scl_rht_curve" ;
        lv2:name "OP5 R KEY CURVE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "-LIN" ;
            rdfs:comment "-LIN" ;
        ], [
            rdf:value 1 ;
            rdfs:label "-EXP" ;
            rdfs:comment "-EXP" ;
        ], [
            rdf:value 2 ;
            rdfs:label "+EXP" ;
            rdfs:comment "+EXP" ;
        ], [
            rdf:value 3 ;
            rdfs:label "+LIN" ;
            rdfs:comment "+LIN" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 139 ;
        lv2:symbol "op5_kbd_rate_scaling" ;
        lv2:name "OP5 RATE SCALING" ;
        lv2:default 3 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 140 ;
        lv2:symbol "op5_amp_mod_sensitivity" ;
        lv2:name "OP5 A MOD SENS." ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 141 ;
        lv2:symbol "op5_key_vel_sensitivity" ;
        lv2:name "OP5 KEY VELOCITY" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 142 ;
        lv2:symbol "op6_eg_rate_1" ;
        lv2:name "OP6 EG RATE 1" ;
        lv2:default 95 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 143 ;
        lv2:symbol "op6_eg_rate_2" ;
        lv2:name "OP6 EG RATE 2" ;
        lv2:default 29 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 144 ;
        lv2:symbol "op6_eg_rate_3" ;
        lv2:name "OP6 EG RATE 3" ;
        lv2:default 20 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 145 ;
        lv2:symbol "op6_eg_rate_4" ;
        lv2:name "OP6 EG RATE 4" ;
        lv2:default 50 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 146 ;
        lv2:symbol "op6_eg_level_1" ;
        lv2:name "OP6 EG LEVEL 1" ;
        lv2:default 99 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 147 ;
        lv2:symbol "op6_eg_level_2" ;
        lv2:name "OP6 EG LEVEL 2" ;
        lv2:default 95 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 148 ;
        lv2:symbol "op6_eg_level_3" ;
        lv2:name "OP6 EG LEVEL 3" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 149 ;
        lv2:symbol "op6_eg_level_4" ;
        lv2:name "OP6 EG LEVEL 4" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 150 ;
        lv2:symbol "op6_operator_output_level" ;
        lv2:name "OP6 OUTPUT LEVEL" ;
        lv2:default 79 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 151 ;
        lv2:symbol "op6_osc_mode" ;
        lv2:name "OP6 MODE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Ratio" ;
            rdfs:comment "Ratio" ;
        ], [
            rdf:value 1 ;
            rdfs:label "Fixed" ;
            rdfs:comment "Fixed" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 152 ;
        lv2:symbol "op6_osc_freq_coarse" ;
        lv2:name "OP6 F COARSE" ;
        lv2:default 1 ;
        lv2:minimum 0 ;
        lv2:maximum 31 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 153 ;
        lv2:symbol "op6_osc_freq_fine" ;
        lv2:name "OP6 F FINE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 154 ;
        lv2:symbol "op6_osc_detune" ;
        lv2:name "OP6 OSC DETUNE" ;
        lv2:default 7 ;
        lv2:minimum -7  ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 155 ;
        lv2:symbol "op6_kbd_lev_scl_brk_pt" ;
        lv2:name "OP6 BREAK POINT" ;
        lv2:default 41 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 156 ;
        lv2:symbol "op6_kbd_lev_scl_lft_depth" ;
        lv2:name "OP6 L SCALE DEPTH" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 157 ;
        lv2:symbol "op6_kbd_lev_scl_rht_depth" ;
        lv2:name "OP6 R SCALE DEPTH" ;
        lv2:default 19 ;
        lv2:minimum 0 ;
        lv2:maximum 99 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 158 ;
        lv2:symbol "op6_kbd_lev_scl_lft_curve" ;
        lv2:name "OP6 L KEY CURVE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "-LIN" ;
            rdfs:comment "-LIN" ;
        ], [
            rdf:value 1 ;
            rdfs:label "-EXP" ;
            rdfs:comment "-EXP" ;
        ], [
            rdf:value 2 ;
            rdfs:label "+EXP" ;
            rdfs:comment "+EXP" ;
        ], [
            rdf:value 3 ;
            rdfs:label "+LIN" ;
            rdfs:comment "+LIN" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 159 ;
        lv2:symbol "op6_kbd_lev_scl_rht_curve" ;
        lv2:name "OP6 R KEY CURVE" ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "-LIN" ;
            rdfs:comment "-LIN" ;
        ], [
            rdf:value 1 ;
            rdfs:label "-EXP" ;
            rdfs:comment "-EXP" ;
        ], [
            rdf:value 2 ;
            rdfs:label "+EXP" ;
            rdfs:comment "+EXP" ;
        ], [
            rdf:value 3 ;
            rdfs:label "+LIN" ;
            rdfs:comment "+LIN" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 160 ;
        lv2:symbol "op6_kbd_rate_scaling" ;
        lv2:name "OP6 RATE SCALING" ;
        lv2:default 3 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 161 ;
        lv2:symbol "op6_amp_mod_sensitivity" ;
        lv2:name "OP6 A MOD SENS." ;
        lv2:default 0 ;
        lv2:minimum 0 ;
        lv2:maximum 3 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 162 ;
        lv2:symbol "op6_key_vel_sensitivity" ;
        lv2:name "OP6 KEY VELOCITY" ;
        lv2:default 6 ;
        lv2:minimum 0 ;
        lv2:maximum 7 ;
	lv2:portProperty lv2:integer ;
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 163 ;
        lv2:symbol "op1_enable" ;
        lv2:name "OP1 ENABLE" ;
        lv2:default 1 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Off" ;
            rdfs:comment "Off" ;
        ], [
            rdf:value 1 ;
            rdfs:label "On" ;
            rdfs:comment "On" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 164 ;
        lv2:symbol "op2_enable" ;
        lv2:name "OP2 ENABLE" ;
        lv2:default 1 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Off" ;
            rdfs:comment "Off" ;
        ], [
            rdf:value 1 ;
            rdfs:label "On" ;
            rdfs:comment "On" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 165 ;
        lv2:symbol "op3_enable" ;
        lv2:name "OP3 ENABLE" ;
        lv2:default 1 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Off" ;
            rdfs:comment "Off" ;
        ], [
            rdf:value 1 ;
            rdfs:label "On" ;
            rdfs:comment "On" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 166 ;
        lv2:symbol "op4_enable" ;
        lv2:name "OP4 ENABLE" ;
        lv2:default 1 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Off" ;
            rdfs:comment "Off" ;
        ], [
            rdf:value 1 ;
            rdfs:label "On" ;
            rdfs:comment "On" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 167 ;
        lv2:symbol "op5_enable" ;
        lv2:name "OP5 ENABLE" ;
        lv2:default 1 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Off" ;
            rdfs:comment "Off" ;
        ], [
            rdf:value 1 ;
            rdfs:label "On" ;
            rdfs:comment "On" ;
        ];
    ] ,
    [
        a lv2:InputPort, lv2:ControlPort ;
        lv2:index 168 ;
        lv2:symbol "op6_enable" ;
        lv2:name "OP6 ENABLE" ;
        lv2:default 1 ;
        lv2:minimum 0 ;
        lv2:maximum 1 ;
        lv2:portProperty lv2:enumeration, lv2:integer ;
        lv2:scalePoint [
            rdf:value 0 ;
            rdfs:label "Off" ;
            rdfs:comment "Off" ;
        ], [
            rdf:value 1 ;
            rdfs:label "On" ;
            rdfs:comment "On" ;
        ];
    ] ;

    doap:name "Dexed" ;
    doap:maintainer [ foaf:name "dcoredump" ] .

